|  |  |  |  |
| --- | --- | --- | --- |
| **carselect Project Status (08/05/2025 - 04:01:34)** | | | |
| **Project File:** | carryselect.xise | **Parser Errors:** | No Errors |
| **Module Name:** | carselect | **Implementation State:** | Programming File Generated |
| **Target Device:** | xc3s400-4ft256 | * **Errors:** | No Errors |
| **Product Version:** | ISE 14.6 | * **Warnings:** | [2 Warnings (2 new)](D://ms/carryselect/_xmsgs/*.xmsgs?&DataKey=Warning) |
| **Design Goal:** | Balanced | * **Routing Results:** | [All Signals Completely Routed](D://ms/carryselect/carselect.unroutes) |
| **Design Strategy:** | [Xilinx Default (unlocked)](Xilinx%20Default%20(unlocked)?&DataKey=Strategy) | * **Timing Constraints:** |  |
| **Environment:** | [System Settings](D://ms/carryselect/carselect_envsettings.html) | * **Final Timing Score:** | 0  [(Timing Report)](D://ms/carryselect/carselect.twx?&DataKey=XmlTimingReport) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Device Utilization Summary** | | | | | [**[-]**](?&ExpandedTable=DeviceUtilizationSummary) |
| **Logic Utilization** | **Used** | **Available** | **Utilization** | **Note(s)** | |
| Number of 4 input LUTs | 19 | 7,168 | 1% |  | |
| Number of occupied Slices | 11 | 3,584 | 1% |  | |
| Number of Slices containing only related logic | 11 | 11 | 100% |  | |
| Number of Slices containing unrelated logic | 0 | 11 | 0% |  | |
| Total Number of 4 input LUTs | 19 | 7,168 | 1% |  | |
| Number of bonded [IOBs](D://ms/carryselect/carselect_map.xrpt?&DataKey=IOBProperties) | 22 | 173 | 12% |  | |
| Average Fanout of Non-Clock Nets | 2.96 |  |  |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Performance Summary** | | | | [**[-]**](?&ExpandedTable=PerformanceSummary) |
| **Final Timing Score:** | 0 (Setup: 0, Hold: 0) | **Pinout Data:** | [Pinout Report](D://ms/carryselect/carselect_par.xrpt?&DataKey=PinoutData) | |
| **Routing Results:** | [All Signals Completely Routed](D://ms/carryselect/carselect.unroutes) | **Clock Data:** | [Clock Report](D://ms/carryselect/carselect_par.xrpt?&DataKey=ClocksData) | |
| **Timing Constraints:** |  |  |  | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Detailed Reports** | | | | | | [**[-]**](?&ExpandedTable=DetailedReports) |
| **Report Name** | **Status** | **Generated** | **Errors** | **Warnings** | **Infos** | |
| [Synthesis Report](D://ms/carryselect/carselect.syr) | Current | Tue 5. Aug 03:57:47 2025 | 0 | [2 Warnings (2 new)](D://ms/carryselect/_xmsgs/xst.xmsgs?&DataKey=Warning) | 0 | |
| [Translation Report](D://ms/carryselect/carselect.bld) | Current | Tue 5. Aug 04:01:15 2025 | 0 | 0 | 0 | |
| [Map Report](D://ms/carryselect/carselect_map.mrp) | Current | Tue 5. Aug 04:01:20 2025 | 0 | 0 | [2 Infos (2 new)](D://ms/carryselect/_xmsgs/map.xmsgs?&DataKey=Info) | |
| [Place and Route Report](D://ms/carryselect/carselect.par) | Current | Tue 5. Aug 04:01:26 2025 | 0 | 0 | [2 Infos (2 new)](D://ms/carryselect/_xmsgs/par.xmsgs?&DataKey=Info) | |
| Power Report |  |  |  |  |  | |
| [Post-PAR Static Timing Report](D://ms/carryselect/carselect.twr) | Current | Tue 5. Aug 04:01:28 2025 | 0 | 0 | [6 Infos (6 new)](D://ms/carryselect/_xmsgs/trce.xmsgs?&DataKey=Info) | |
| [Bitgen Report](D://ms/carryselect/carselect.bgn) | Current | Tue 5. Aug 04:01:32 2025 | 0 | 0 | [1 Info (1 new)](D://ms/carryselect/_xmsgs/bitgen.xmsgs?&DataKey=Info) | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Secondary Reports** | | | [**[-]**](?&ExpandedTable=SecondaryReports) |
| **Report Name** | **Status** | **Generated** | |
| [WebTalk Report](D://ms/carryselect/usage_statistics_webtalk.html) | Current | Tue 5. Aug 04:01:33 2025 | |
| [WebTalk Log File](D://ms/carryselect/webtalk.log) | Current | Tue 5. Aug 04:01:34 2025 | |

**Date Generated:** 08/05/2025 - 04:01:34